Current Help System: Tutor Translator (View Core Help)

### Pick (Uncompensated Point) Measurement Commands

PC-DMIS does not have MPICK equivalent measurement command. The command can be approximately translated as a measured point (compensated) and extracting uncompensated coordinates using the RAWHIT operator.

MPICK (MEMORY [10], 1) translates to è

ASSIGN/E.BADMEAS=0

PNT14 = FEAT/POINT,RECT

THEO/<10,120,30>,<0,0,1>
ACTL/<10,120,40>,<0,0,1>
MEAS/POINT,1
MOVE/POINT,<12,123,35>
HIT/BASIC,<10,120,30>,<10,120,30>,USE THEO = NO
MOVE/POINT,<12,123,350>
ENDMEAS/

ASSIGN/COMP_POINT = PNT14.RAWHIT[1].XYZ

PNT15 = GENERIC/POINT,DEPENDENT,RECT,$

NOM/XYZ,<PNT14.TX,PNT14.TY,PNT14.TZ>,$
MEAS/XYZ,<COMP_POINT.X,COMP_POINT.Y,COMP_POINT.Z>,$
NOM/IJK,<PNT14.TI,PNT14.TJ,PNT14.TZ>,$
MEAS/IJK,<PNT14.I,PNT14.J,PNT14.K>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PNT15")
ASSIGN/E.WM1.TYPE = 115
ASSIGN/E.MEMORY[10] = E.WM1
…
… Evaluation commands.
…