Current Help System: PC-DMIS Vision (View Core Help)

#### Edge Point with NC-100

NC-100 Edge Point Auto Feature

The Edge Point measurement option allows you to define a point measurement that is to be taken on the part's edge.

There are four types of edge measurements. These include:

- EDGE NORMAL

- EDGE DELTAZ

- EDGE HIGH

- EDGE BIGHOLE

They require different input-output parameter settings and different theoretical definitions in the PC-DMIS command.

Point acquired by vision system

To access the Edge Point option:

1. Access the Auto Features dialog box (
   Insert | Feature | Auto | Point | Edge).

2. Select the Edge Point auto feature type.

The Edit window command line for a sample Edge Point would read:

F_ID=AUTO/EDGE NORMAL, SHOWHITS = Y/N, SHOWALLPARAMS = Y/N,
THEO/ TX,TY,TZ,TI,TJ,TK
ACTL/ X,Y,Z,I,J,K
TARG/ targX,targY,targZ,targI,targJ,targK
THEO_THICKNESS = n ,TOG3 ,EDGE THEO_THICKNESS = .n
AUTOMOVE=TOG , DISTANCE = n,
SURFACE NORMAL = I,J,K, DEPTH = n

More:

Edge Point Type Definition

Edge Point Field Definition

Measuring an Edge Point with NC-100