Current Help System: PC-DMIS Vision (View Core Help)

#### Round Slot Field Definitions with NC-100

Many of the definitions are already covered in the "Round Slot Field Definitions" topic in the "Creating Auto Features" section. The following definitions are added or changed when using a NC-100 video probe :

SHOWHITS = This is a toggle field. It toggles from YES to NO and determines if hits will be displayed with this feature. This is not currently available.

SHOWALLPARAMS = This is a toggle field. It toggles from YES to NO as to displaying all the parameters on the feature.

ACTL_THICKNESS = This value indicates the keyed in offset thickness of the measured data. Positive or negative values can be used.

See the "Common Auto Feature Dialog Box Options" topic in the "Creating Auto Features" section for general guidelines on measuring all Auto Feature types.