Current Help System: PC-DMIS Vision (View Core Help)

#### Measuring an Edge Point with NC-100

PC-DMIS allows these methods for measuring an edge point with the NC-100 video probe. They are listed below:

Using Keyed in Data

This is covered in "Using Keyed in Data for an Edge Point" in the "Creating Auto Features" section.

Using Surface Data on the Screen

This is covered in "Using Surface Data on the Screen for an Edge Point" in the "Creating Auto Features" section.

Using Wire frame Data on the Screen

This is covered in "Using Wire frame Data on the Screen for an Edge Point" in the "Creating Auto Features" section.

Note: The mouse cannot be used in the Graphics Display window if CAD data is unavailable.

Note: PC-DMIS assumes that the normal surface and the measurement surface are perpendicular.