Current Help System: PC-DMIS CMM (View Core Help)

#### Center Basic Scan - Measured Point Method

To generate the Center scan without the use of CAD data:

1. Select the desired point in the list.

2. Take a hit on the part. This will fill up the values for that point.

The CutVec is the normal vector of the plane in which the probe remains free while centering is done by the controller. The Init Vec is the initial approach vector at the Start Point.