## Configuring the Romer Infinite Arm with a Perceptron Contour Sensor

This section contains supplemental material to the standard WinRDS documentation for your Romer Infinite Arm using a Perceptron Contour Sensor. For additional information please consult the other manuals.

To configure your Infinite Arm to use a Perceptron Contour Sensor follow these steps:

1. Romer Infinite Arm Setup

2. Setting WinRDS Environment Variables

3. Install PC-DMIS for Romer

4. Connect the Contour Sensor Controller Box

5. Configure the Network Card

6. Attach Your Contour Sensor

7. Complete the PC-DMIS Configuration

8. Verify Sensor Installation