### Reflex Interface

The Reflex interface is used with a Reflex controller. This interface is intended for use on a manual Gage 2000 machine with the Reflex box in Pass Through Mode. There are 2 “smart cards” that are inserted in the controller. The upper one is the storage card, where the programs are stored. After turning on the Reflex Controller, you will notice the following screens:

Before starting PC-DMIS, rename the Reflex.dll to interfac.dll.

The Machine Option dialog box has four tabs for the Reflex interface:

Controller tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 9600 Baud, No parity, 8 data bits, and 1 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).