### Manmora Interface

The Manmora interface is used with manual Mora machines. This machine has a GEMODEK type MR01 counter box with XYZ readout with some control/setup/send options. See the MIIM for additional configuration and testing information.

Before starting PC-DMIS, rename the Manmora.dll to interfac.dll.

The Machine Option dialog box has four tabs for the Manmora interface:

Controller tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 9600 Baud, No parity, 8 data bits, and 2 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Resolution tab

See the "Setting the Axes Scale Factor" topic. Default is X=1.0, Y=1.0, Z=1.0.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).