### Multiple Arm Program Execution

Unless you choose to execute just the commands assigned to a particular arm, when you execute the part program, the program flow continues as it normally does from the top of the Edit window to the bottom, and each arm executes the commands assigned to it.

Note: When executing in multiple arm mode, Arm2 will always run a little behind Arm1. This type of delay is normal.