### Renishaw Interface

The Renishaw interface communicates with the Renishaw installed software (V4.0 or later). There is also a special interface card (or USB module) that is used to communicate via optical link with the UCC1 controller. The software and interface card must be obtained from Renishaw.

Before starting PC-DMIS, rename the Renishaw.dll to interfac.dll.

The Machine Option dialog box has two tabs for the Renishaw interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).