#### Read Point

F_ID= FEAT/ POINT, TOG1
THEO/ x, y, z, i, j, k
ACTL/ x, y, z, i, j, k
READPOINT

The Read Point command creates a point feature at the current location of the probe. PC-DMIS will then store the values of the point that is read.

Important: If you execute this type of point feature in offline mode and the feature follows a MODE/MANUAL command, it will copy the theoretical vector and position to the measured vector and position; otherwise, the value will come from the current probe position.

See "Creating a ReadPoint from the Probe's Position" in the "Creating Generic Features" section for additional information.