#### Machine Commands

The Machine Commands list displays any moves and hits for the current feature (or the feature about to be measured). This information is only available if the program is stopped during execution, either by error or by the operator. Execution of the part program can be resumed by highlighting the desired hit (or move) from the Machine Commands list box and selecting the Continue button.

Example: If a clearance move command was programmed with the wrong X, Y, or Z, then during the execution of that move, you might get a motion error. To continue:
Pull down the Machine Commands drop-down list.
Select the command following the offending move.
Press the Continue button.