#### Meas All Once

If you select the Meas All Once check box,

- PC-DMIS will remeasure all the input features at least once in DCC mode.

- They will be measured in the order specified by the iterative alignment command in the Edit window.

- PC-DMIS will display which feature is about to be measured in a message box.

- Before accepting the move, ensure that the probe can reach the indicated feature(s) without colliding with the part.

- Stored moves found before or after each feature will not be executed.

- After all the features have been measured at least once, remeasurement of the features will continue for measured point types of features and those points that missed their Point Target Radius target (see "Point Target Radius").

Note: PC-DMIS will not measure circles more than one time while in this mode since their location never changes.