#### Step 4 - Take the First Manual Hit

You will be prompted through the process of measuring three manual hits through a series of message boxes. Three hits are required to fully define the orientation of this rack in the machine’s XY plane. It is not necessary to align the rack to any single axis, as the manual hits will identify any rotation involved. Follow the prompts and take the needed hits as shown in the pictures for each hit.

The first manual hit is taken in the XY plane, on the vertical face in front of the rack between Port 1 and Port 2.

Prompt for the First Hit on the Front Face:

PC-DMIS MESSAGE: Open all lids and remove any probe from port 1. When ready, please take a hit in the center of the vertical face between ports 1 and 2.

Using your machine's jog box, measure the first hit on the front face between Port 1 and Port 2. |

Next Step