### Supported Interfaces

Not all interfaces support the ON ERROR command. Consult the following table to see if your interface is supported.

- If your interface is listed, an X indicates what error type is supported by that interface.

- If your interface isn't listed, then it's not able to use the ON ERROR command.

Supported Interfaces | Unexpected Probe Hit | Missed Probe Hit | Reflector Not Found
B&S Standard | X | X |
Dea |  | X |
Elm | X | X |
Federal/Renault | X | X |
Johansson | X | X |
Leica Tracker |  |  | X
Leitz | X | X |
LK Direct (also known as LKRS232) | X | X |
LK Driver | X | X |
Metrolog | X | X |
Mitutoyo Bright | X | X |
Mitutoyo | X | X |
Mora | X | X |
Omnitech | X | X |
Renishaw | X | X |
Sharpe | X | X |
Sheffield | X | X |
Wenzel | X | X |
Zeiss | X | X |