#### Step 5 - Take the Second Manual Hit

The second manual hit is taken in the Z direction, on the horizontal face on top of the rack between Port 2 and Port 3.

Prompt for the Second Hit on the Top:

PC-DMIS MESSAGE: Please take a hit on top of the metallic docking plate in the middle between ports 2 and 3.

Using your machine jog box, measure the second hit on the top metal surface between Port 2 and Port 3. |

Next Step