Current Help System: PC-DMIS Laser (View Core Help)

#### Cylinder Command Mode Text

Sample Stud Cylinder

CYL1 =FEAT/LASER/CYLINDER/DEFAULT,CARTESIAN,OUT

THEO/<3.1425,2.7539,0>,<0,0,1>,0.25,0.25

ACTL/<3.1425,2.7539,0>,<0,0,1>,0.25,0.25

TARG/<3.1425,2.7539,0>,<0,0,1>

DEPTH=0

MEASURE MODE=STUD

CENTER OFFSET=0

SEARCH LENGTH=0

SHOW FEATURE PARAMETERS=NO

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=COP1

HORIZONTAL CLIPPING=0.0787,VERTICAL CLIPPING=0.0787

Sample Inner Cylinder

CYL2 =FEAT/LASER/,CYL2=FEAT/CYLINDER,CARTESIAN,IN

THEO/<1.895,1.91,1>,<0,0,1>,1.895,7

ACTL/<1.895,1.91,1>,<0,0,1>,1.895,7

TARG/<1.895,1.91,1>,<0,0,1>

DEPTH=3

SHOW FEATURE PARAMETERS=YES

SURFACE=THEO_THICKNESS,1

MEASURE MODE=NOMINALS

RMEAS=NONE,NONE,NONE

AUTO WRIST=NO

GRAPHICAL ANALYSIS=NO

FEATURE LOCATOR=NO,NO,""

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=25,OVERSCAN=2,EXPOSURE=18

FILTER=NONE