Current Help System: PC-DMIS Laser (View Core Help)

## TCP/IP Pointcloud Server

PC-DMIS can send your pointcloud data to a custom-built third-party software. It uses a TCP/IP communication protocol to do this. To establish the connection, your custom application must be able to load a dynamic link library (dll) file named PcDmisPointCloudClientDll.dll. You can request this file from Hexagon Metrology's Customer Support.

Once your application loads the dll file, click on one of these TCP/IP Pointcloud server icons available from PC-DMIS's Pointcloud toolbar to establish the connection:

TCP/IP Pointcloud Server Connection with Local Copy - This establishes the connection with the client, sends the point cloud data directly to the client, and when the scan finishes, the point cloud data remains inside the part program.

TCP/IP Pointcloud Server Connection without Local Copy - This establishes the connection with the client, sends the point cloud data directly to the client, and when the scan finishes, the point cloud data is deleted from the part program.