Current Help System: PC-DMIS Laser (View Core Help)

## Polygon Command Mode Text

The Polygon command inside the Edit window’s Command Mode looks like this:

POL1 =FEAT/LASER/POLYGON,CARTESIAN

THEO/<1.0379,1.9488,0.5906>,<0,0,1>,<0.8660254,-0.5,0>,0.5118

ACTL/<1.0379,1.9488,0.5906>,<0,0,1>,<0.8660254,-0.5,0>,0.5118

TARG/<1.0379,1.9488,0.5906>,<0,0,1><0.8660254,-0.5,0>

NUMSIDES=6

DEPTH=0

SHOW FEATURE PARAMETERS=NO

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=30,OVERLAP=0.0394

OVERSCAN=0.0787,EXPOSURE=35

FILTER=NONE

PIXEL LOCATOR=GRAY SUM,Min=30,Max=300

CLIPPING TOP=100,BOTTOM=0,LEFT=0,RIGHT=100

RINGBAND=OFF