Current Help System: PC-DMIS Portable (View Core Help)

### Step 4: Complete the PC-DMIS Configuration

You are now ready to start PC-DMIS. After launching PC-DMIS, open a new part program and follow these steps to complete the configuration:

1. Open the Setup Options dialog box by pressing F5.

2. Select the Laser tab.

3. Type the path to the CSGMain.bin file in the Sensor Binary File edit box. This is normally installed with PC-DMIS into the Perceptron subdirectory of the main PC-DMIS installation. Alternatively, you can use the Browse button to locate this file.

4. Click OK on the Setup Options dialog box.

To verify that the sensor is working in PC-DMIS, close down PC-DMIS and restart. This will ensure that all necessary information is written to the system registry.

Next Step ...