Current Help System: PC-DMIS Portable (View Core Help)

#### Step 1: Install PC-DMIS Portable for Total Station

To install PC-DMIS Portable for the Leica Total Station, simply insert your portlock into your computer and run the PC-DMIS setup program. Your portlock must be configured to use the Total Station interface. Once you have run the setup program, simply run PC-DMIS and you are ready to start measuring.

Note: If you are an AE and have a portlock programmed for all interfaces, you can run the PC-DMIS setup program with the following startup option to get an install of PC-DMIS as if your portlock had been programmed specifically for Total Station. The word "Interface" is case sensitive.
/Interface:leicatps
This will add /portable:leicatps switches onto the offline and online shortcuts as well as copy the custom layouts associated with the Total Station.