Current Help System: PC-DMIS Portable (View Core Help)

### Resetting the Tracker Beam (6dof devices only)

If the laser beam from the Leica Tracker is broken and the tracker is unsuccessful in following the reflector or T-Probe location, it might be necessary to reset the position to which the laser is pointing. This allows you to recapture the beam at a known location.

This is mainly used for LT trackers which do not have an integrated ADM.

You can reset the laser to point to one of two positions:

- Birdbath: Select Tracker | Go Birdbath to reset the laser to point to the Birdbath position. This is used when working with reflectors.

- 6DoF: Select Tracker | Go 6DoF 0 Position to reset the laser position by pointing to the predefined T-Probe 0 position. This will allow you to catch the beam at that location. This is used when working with a T-Probe.

Use these options to catch the reflector again and bring the reflector or T-Probe to a stable position, this will re-establish a distance via ADM and allows you to continue.