Current Help System: PC-DMIS Settings Editor (View Core Help)

### FCF ID Generic

Determines if feature control frames ID labels are displayed with a generic value (typically "FCF") for all FCF label types. When this value is set to FALSE (0), FCF labels will be displayed based on the feature type (Circularity = FCFCIRTY, Coaxiality = FCFCOAX, Flatness = FCFFLAT, etc.)

Entry Name: FetIDGeneric

Entry Type: Whole Number to specify Generic (1) or By Type (0). Default value is 0.