Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Shutter Time To Fire Nth

This value provides the delay (in milliseconds) that PC-DMIS waits before issuing the point detect command when PC-DMIS detects that the ROI (Region of Interest), that is not the FIRST ROI, is ready to fire. This delay gives the stage a chance to settle before firing the point detection. The recommended setting is 200.

This value is only evaluated when "AutoShutterEnable" is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

Entry Name: AutoShutterTimeToFireNth

Entry Type: Whole Number to specify milliseconds. Default value is 200.