Current Help System: PC-DMIS Settings Editor (View Core Help)

### Connect Time Arm (1-4)

This value is the number of milliseconds that PC-DMIS will delay before attempting a TCP/IP connection to the given arm (1-4) arm to the current (master) computer. Values can be provided for Arm 1-4 respectively. This value is only used when ConnectionTypeArm(1-4) for the relevant arm is set to 1(Remote Connection) and this is the Master computer set with a value of 1 for Mode.

Entry Name: ConnectTimeArm(1-4)

Entry Type: Character String specifying milliseconds. Default value is 500

required to change entry.