Current Help System: PC-DMIS Settings Editor (View Core Help)

### Valisys TCP IP Port

Specifies Valisys server port that PC-DMIS connects to when using TCP/IP to establish a connection. A value greater then 5000 should be used. The Valisys host port must be set to the same value for communication to work.

Note: When TCP/IP is being used there should not be an entry for ValisysCommPort.

Entry Name: ValisysTCPIPPort

Entry Type: Character String to specify the TCP/IP port. Default value is 55555.