Current Help System: PC-DMIS Settings Editor (View Core Help)

### External Probehead Protocol

This value sets the communications protocol for the serial connection to the probe head. It specifies the comm port, baud rate, parity, data bits and stop bits settings. If the port is set to COM0, PC-DMIS will not attempt to open or use the external probe head connection even if the type is set to a supported value.

Entry Name: ExternalProbeheadProtocol

Entry Type: Character String specifying probe head protocol. Default value is “COM2 9600 E,7,1”.