Current Help System: PC-DMIS Settings Editor (View Core Help)

### PTP_Read Pos

Allows you to define the default value for the Read Pos option that will be used when an Auto Feature is created. The Read Pos option is used right before measuring a feature. PC-DMIS will stop above the surface and will display a message, asking if you want to use the current data. This functionality is active when this value is set to TRUE.

Entry Name: PTP_R eadPos

Entry Type: True/False value. Default value is FALSE.

Note: Read Pos is only available in DCC Mode.

See the "Read Pos" topic for more information.