Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Frequency

Controls the internal sensor frequency (pulses per second) of the probe. The maximum sensor frequency is 30 pulses per second. Using this value means that you will collect a lot of data. The minimum setting is 1. A setting of 15 may be a good balance between speed and accuracy.

Entry Name: SensorFrequency

Entry Type: Whole Number specifying pulses per second. Default value is 0.