Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Shutter Stage Drift Retries

Determines the number of times that PC-DMIS Vision will retry point detection before a failure is reported. If the stage is not stable, then point detection is not reliable. During point detection, if the stage drifted between the time the point detect command is issued and the time the point detect command completes and returns the points, the point detection is retried.

This value is only evaluated when "AutoShutterEnable" is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

Entry Name: AutoShutterStageDriftRetries

Entry Type: Whole Number to specify number of retries. Default value is 0.