Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Rotation Comp Enabled

Stores whether previously the calibrated camera to stage rotation was compensated. When this value is set to TRUE (1), rotation was compensated.

Entry Name: ProbeQualVisionOpticsCalRotationCompEnabled

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.