Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Targ XYZ_0

Provides the default "X" or "R" (radius) value for the center location for all auto features created with the NC-100 video probe. The value will represent X value when the "Cartesian" value is set to TRUE (1), and R when it is set to FALSE (0).

Entry Name: DccTargXYZ_0

Entry Type: Real Number to specify the X or R value. Default value is 0.