Current Help System: PC-DMIS Settings Editor (View Core Help)

### UV Scan V Start

Defines the start location of the area on the scan surface in the V direction (approximate Y Direction) that will be included as part of the UV Scan. For example, a value of .1 would begin scanning 10% of the way in the V direction.

Entry Name: UVScanVStart

Entry Type: Real Number specifying portion of the whole surface (1). Default value is 0.1.