Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Mode

Specifies the type of probing cycle used. The most common cycle is deflection mode (DFL). Other cycles, such as soft probing (SFT), may also be supported by some analog probes/controllers. In some cases the probe/controller may not have multiple modes and this value is ignored.

Entry Name: ProbeMode

Entry Type: Character String for probing cycle (e.g. DFL, SFT, etc). Default value is DFL.