Current Help System: PC-DMIS Settings Editor (View Core Help)

### Wait For Ack In Master Slave Mode

Determines whether acknowledgment (ACK) is used for communication between dual arm machines. Both the master and slave computer must be set to the same value for proper communication. When the value is set to TRUE (1), both computers will acknowledge that strings that are passed between the two machines are sent and received correctly. This ensures that the needed stings are available on the each machine and that they are received in the correct order. Using ACK is beneficial for poorly performing networks.

Entry Name: WaitForAckInMasterSlaveMode

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.

Administrator permission is