Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Body Axis

Specifies the axis to be used with the Body Axis Direction 1 Technique. The available axes are X, Y, and Z. The cut plane that your probe will crisscross will be parallel to this axis.

Entry Name: ScanDialogBodyAxis

Entry Type: Whole Number specifying axis number. Default value is 0.

Axis Key

0 | X
1 | Y
2 | Z