Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Tol Above

Determines the number of pixels in the image that the next pixel is allowed to rise and still be accepted as part of a continuous line. The value indicates the number of pixels above the current pixel that the filter will still use. The Long Line value uses this value for measuring spheres and some cylinders.

Entry Name: SensorTolAbove

Entry Type: Real Number to specify number of pixels. Default value is 0.