Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Targ XYZ _1

Provides the default "Y" or "A" (angle) value for the center location for all auto features created with the NC-100 video probe. The value will represent Y value when the "Cartesian" value is set to TRUE (1), and A when it is set to FALSE (0).

Entry Name: DccTargXYZ_1

Entry Type: Real Number to specify the Y or A value. Default value is 0.