Current Help System: PC-DMIS Vision (View Core Help)

#### Square Slot/Gap & Flush with NC-100

NC-100 Square Slot/Flush & Gap Auto Feature

The Square Slot option allows you to define a square slot measurement or a Gap & Flush measurement. See "Square Slot and Gap & Flush Type Definition with NC-100" for the available measurement types.

The Square Slot can be measured using the points inside the ROI and along the slot contour.

Square slot measurement

To access the Square Slot option:

1. Access the Auto Features dialog box (
   Insert | Feature | Auto | Square Slot ).

2. Select the Square Slot auto feature type.

The Edit window command line for a sample Square Slot would read:

F_ID=AUTO/SQUARE SLOT, SHOWHITS=Y/N, SHOWALLPARAMS=Y/N
THEO/ TX,TY,TZ,TI,TJ,TK,TWIDTH,TLENGTH,
ACTL/ X,Y,Z,I,J,K, WIDTH, LENGTH,
TARG/ targX,targY,targZ,targI,targJ,targK
THEO_THICKNESS = n, TOG1
AUTO MOVE = Y/N, DISTANCE = n

The Edit window command line for a sample Gap & Flush would read:

F_ID=AUTO/GAP DELTAZ, SHOWHITS=Y/N, SHOWALLPARAMS=Y/N
THEO/ TX,TY,TZ,TI,TJ,TK,TGAP,TFLUSH
ACTL/ X,Y,Z,I,J,K,GAP,FLUSH
TARG/ targX,targY,targZ,targI,targJ,targK
THEO_THICKNESS = n, TOG1, TOG2
AUTO MOVE = Y/N, DISTANCE = n, DEPTH = n, DEPTH2 = n

More:

Square Slot/Gap and Flush Type Definition

Square Slot/Gap and Flush Field Definition

Measuring a Square Slot with NC-100

Specific Functions for Flush and Gap Features

Feature Type for a Square Slot and Gap Flush Measurements