Current Help System: PC-DMIS Vision (View Core Help)

### Step 5: Perform Calibrations

Before you begin measuring with your Vision probe, in most cases it is necessary to perform the various calibration procedures on your machine. This includes:

- Optical Center

- Optics

- Illumination

- Probe Offset

See the "Calibrating Vision Probes" topic for information on calibrating your Vision probe. Also see "Calibrating the Vision Stage" for information on Vision stage calibrations.

Next Step...