Current Help System: PC-DMIS Vision (View Core Help)

#### Step 4: Fill out the Measure Probe Dialog Box

In the Measure Probe dialog box, you will now see values displayed in the various boxes. These are the parameter settings that PC-DMIS will used during the measurement process.

You can accept these default values or change them to meet your specific needs.

1. Select Calibrate NC-100 Artifact option button from the Type of Operation area.

2. Select the Manual, DCC, or ManDCC option.

Note: Even if DCC or ManDCC mode is selected, PC-DMIS will require you to manually take hits on the calibration tool.

Next Step...