Current Help System: PC-DMIS Vision (View Core Help)

#### Using 2D Profile Edge Tracer

You can program a 2D Profile feature simply by double-clicking near the edge of the feature in the Live View. PC-DMIS Vision, will automatically trace around the edge of the feature, moving the machine stage on a DCC machine if necessary.

Rules for Clicks to Start Edge Tracer

- If you just double-click, PC-DMIS Vision will travel around the edge in an counter-clockwise direction, trying to return to the start position.

- If you first single click a point before double clicking, that first clicked point will be your start point and the double click point will be your targeted end point.

- If you click two points before double clicking, the first click is the start point, and the second click dictates the direction in which the trace will proceed. The double-click position will be the end point.

Once the edge trace is completed, you can then adjust the nominal segments as necessary.