Current Help System: PC-DMIS CMM (View Core Help)

### Performing a Grid Advanced Scan

Grid Scan dialog box

The Insert | Scan | Grid scan, similar to the UV scan, lets you to easily create a grid of points within a visible rectangle and then project those points down on top of any selected surfaces. UV and Grid scans are similar in the way that they construct and space points within a selected area. However, the orientation of the points with respect to the a CAD model's orientation differs.

Consider these two figures:

Figure 1 - UV Scan on 2D Rotated Part | Figure 2 - Grid Scan on 2D Rotated Part

Figure 1 shows a UV scan on the top surface of a 2D rotated sample block. Figure 2, shows the same block with a Grid scan. Notice how the UV axes in figure 1 are in line with the XY axes of the selected surface. The Grid scan, on the other hand, does not do this; instead, the points remain aligned with the rectangle view. When created, the Grid scan creates the points where they fall on the selected surfaces, regardless of part orientation

To Create a Grid Scan

1. Enable a TTP Probe.

2. Place your CAD model in Solid mode.

3. Place PC-DMIS into DCC mode.

4. Access the Grid Scan dialog box (Insert | Scan | Grid).

5. Type the name of the scan in the ID box if you want to use a custom name.

6. Drag a rectangle on the screen over the surface or surfaces you want to include in your scan. This rectangle defines the boundary for the scan.

   Example rectangle taking in several surfaces

7. In the Graphics tab, select the Select check box.

8. Click the surface or surfaces you will scan. PC-DMIS highlights the selected surfaces as you select them.

   An example selected surface, highlighted in red

9. Select the appropriate type of hits to take from the Hit Type list in the Hit Controls area. You can select either Vector or Surface.

10. In the Grid Scan Settings area, define how many hits in the A and B directions will get spaced and dropped onto the selected surface(s).

13. Modify any other options as needed. Only MASTER can be selected from the Nominals list.

14. Select the Generate button in the Theoretical Path area, Path Definitions tab to generate a preview of the scan on the CAD model in the Graphics Display window. PC-DMIS will draw points on the CAD model. It will not draw points on any surface you did not select, even if the boundary of the rectangle includes other surfaces.

    Example showing generated points. Notice that the points only appear on the selected surface (red), even though several other surfaces (blue) are bounded by the rectangle.

15. If needed, you can delete individual points by selecting them one at a time from the Theoretical Path area and pressing the DELETE key.

16. If needed, make any modifications to your scan.

17. Click the Create button. PC-DMIS inserts the scan into the Edit window and draws the route the probe will take on the surface of the model in the Graphics Display window.