### KD - Set nominal soft probe deflection

The KD command sets the nominal soft probe deflection to be used.

Command Format

MLString "KD p1"

Examples

1. MLString "KD 0.05" -

   Set the nominal soft probe deflection to 0.05 units.

Input

- p1 = nominal soft probe deflection (Numeric; optional)

The optional numeric parameter p1 specifies the nominal soft probe deflection in current units. This value must be positive.

If p1 is not specified then the current setting for nominal soft probe deflection is returned. The default value after initialization (IL) is 0.05".

Results

If a value is specified, the nominal soft probe deflection is set to this value except as noted above. If a value is not specified then the current value is returned to variable S7.

Skip Action

Executed normally.

Error Messages

- MLB-090 DCC is not available.