### MP-515 IEEE 488 initialization failure

On an MP-30 system there is an IEEE addressing or transmission error. There is a faulty IEEE chip or control board. It has failed to:

- Set up a talk address or a listen address, or

- Put the chip in talker-only, listener-only, talker-active, or listener-active modes.

Refer to MP Error Codes for additional information.

What you should do

1. Call your Giddings & Lewis service representative.