###

### Basic Measurement Format for a Square Slot

The minimum number of hits for a square slot is five. | Feature_name=FEAT/SLOT,TOG1,TOG2 THEO/TX,TY,TZ,TI,TJ,TK,SI,SJ,SK,TW,TL ACTL/X,Y,Z,I,J,K,MI,MJ,MK,W,L MEAS/SLOT,TOG3,TOG4 ...
ENDMEAS/

T OG1= This field can be toggled between RECT / POLR.

TOG2= This field can be toggled between IN / OUT.

TX,TY,TZ - Theoretical XYZ

TI,TJ,TK - Theoretical IJK vector

SI,SJ,SK - Theoretical IJK slot vector

TW - Theoretical width

TL - Theoretical length

X,Y,Z - Actual measured XYZ

I,J,K - Actual measured IJK

MI, MJ,MK - Measured IJK slot vector

W - Actual measured width

L - Actual measured length

TOG3= This value is user editable and is determined by the feature being measured. The HIT line is varied, based on the number of hits set up by the user. For example, 5 hits = 6 HIT/BASIC lines.

TOG4= This value lets you choose the reference type for the slot.

...= As many hits as are necessary are entered at the ellipsis.