### Embboard Interface

The Embboard interface is used with Brown & Sharpe manual machines with an internal embedded controller card. This is a full-length card located in your PC with the address set to 300h. You must ensure that this address is not used by another board in the system (some network cards use this address).

Before starting PC-DMIS, rename the embboard.dll to interfac.dll.

The Machine Option dialog box has three tabs for the Embboard interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Resolution tab

See the "Setting the Axes Scale Factor" topic. Default is X=1.0, Y=1.0, Z=1.0.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).