### A List of Available Data Types

This list of data types displays the data type names in alphabetical order, their associated type numbers, descriptions, index values and value strings as appropriate. When using data types inside VB scripts in template events and rules, you may need to use the data type number as not all script locations accept the enumerated data type value. To view the list of items starting with that letter, click on a link below. Some of the categories are quite large and may take a few seconds to load. Click on the same link again to collapse the items for that letter.

[ A
| B
| C
| D
| E
| F
| G
| H
| I
| J
| K
| L
| M
| N
| O
| P
| Q
| R
| S
| T
| U
| V
| W
| X
| Y
| Z
]

-Z-

Number | Data Type Name | Data Type Description | Index | Value String
148 | Z_OFFSET | Z Offset for loops |  |
404 | ZONES | For SPC |  |

-Y-

Number | Data Type Name | Data Type Description | Index | Value String
147 | Y_OFFSET | Y Offset for loops |  |

-X-

Number | Data Type Name | Data Type Description | Index | Value String
146 | X_OFFSET | X Offset for loops |  |

-W-

Number | Data Type Name | Data Type Description | Index | Value String
322 | WAVE_FILE | Feature Locator Wave File |  |
137 | WEIGHT | Weight value for Best Fit alignments |  |
154 | WORK_PLANE | Workplane |  |

-V-

Number | Data Type Name | Data Type Description | Index | Value String
319 | V_HITS | Number of V points for surface |  |
363 | VIDEO_GAIN |  |  |
366 | VIDEO_LASERLIGHT1 |  |  |
367 | VIDEO_LASERLIGHT2 |  |  |
365 | VIDEO_LEDLIGHT |  |  |
370 | VIDEO_LSEG |  |  |
364 | VIDEO_OFFSET |  |  |
371 | VIDEO_XSEG |  |  |
369 | VIDEO_YEND |  |  |
368 | VIDEO_YORIGIN |  |  |
372 | VIDEO_YSEG |  |  |
512 | VOID_DETECT | Turn off void detection | 0 | "YES" or "NO"

-U-

Number | Data Type Name | Data Type Description | Index | Value String
318 | U_HITS | Number of U points for surface |  |
417 | U_L_BOUNDS | For SPC |  |
406 | UCL_LCL | For SPC |  |
172 | UNIT_TYPE | Unit type (inch / mm) |  |
211 | UP_FORCE | Up force for option probe object |  |
127 | UPDATEVEC_I | Update vector i |  |
128 | UPDATEVEC_J | Update vector j |  |
129 | UPDATEVEC_K | Update vector k |  |
431 | USE_3DFILTER |  |  |
139 | USE_AXIS | Flag for iterative alignments and start TP dimension |  |
753 | USE_AXIS2 |  |  |
541 | USE_HSSDAT |  |  |
542 | USE_STARTENDDELAY |  |  |
281 | USE_THEO | BRN added 5/2/2002 |  |
44 | USEPIN_TYPE | Use pin vector or normal vector |  |
738 | USETWODEVIATIONS |  |  |

-T-

Number | Data Type Name | Data Type Description | Index | Value String
345 | T_VALUE | T value on hits |  |
572 | TARG_A |  |  |
590 | TARG_EA |  |  |
591 | TARG_EH |  |  |
589 | TARG_ER |  |  |
516 | TARG_EX | Target endpoint x component |  |
517 | TARG_EY | Target endpoint y component |  |
518 | TARG_EZ | Target endpoint z component |  |
573 | TARG_H |  |  |
31 | TARG_I | Target i - vector |  |
32 | TARG_J | Target j - vector |  |
33 | TARG_K | Target k - vector |  |
571 | TARG_R |  |  |
587 | TARG_SA |  |  |
588 | TARG_SH |  |  |
586 | TARG_SR |  |  |
513 | TARG_SX | Target startpoint x component |  |
514 | TARG_SY | Target startpoint y component |  |
515 | TARG_SZ | Target startpoint z component |  |
19 | TARG_X | Target x - centroid |  |
20 | TARG_Y | Target y - centroid |  |
21 | TARG_Z | Target z - centroid |  |
557 | TARGET_BLOB_TYPE |  |  |
282 | TARGET_COLOR | Vision Target Color |  |
474 | TARGET_DIRECTION |  |  |
520 | TARGET_EDGE_ANGLE |  |  |
508 | TARGET_EDGE_DENSITY |  |  |
712 | TARGET_EDGE_EDGEDETECT |  |  |
538 | TARGET_EDGE_EDGENUM |  |  |
537 | TARGET_EDGE_EDGESELECT |  |  |
717 | TARGET_EDGE_GRADIENT |  |  |
711 | TARGET_EDGE_HEIGHT |  |  |
505 | TARGET_EDGE_ILLUM |  |  |
475 | TARGET_EDGE_POLARITY |  |  |
504 | TARGET_EDGE_SIZE |  |  |
507 | TARGET_EDGE_STRENGTH |  |  |
506 | TARGET_EDGE_TOL |  |  |
509 | TARGET_EDGE_TYPE |  |  |
549 | TARGET_EDGE_UNDERSCAN |  |  |
710 | TARGET_EDGE_WIDTH |  |  |
715 | TARGET_FILTER_AREA |  |  |
716 | TARGET_FILTER_AREA_SIZE |  |  |
713 | TARGET_FILTER_CLEAN |  |  |
714 | TARGET_FILTER_CLEAN_STRENGTH |  |  |
561 | TARGET_FILTER_OUTLIER |  |  |
562 | TARGET_FILTER_OUTLIER_ DISTANCE_THRESHOLD |  |  |
599 | TARGET_FILTER_OUTLIER_ STD_DEV_THRESHOLD |  |  |
523 | TARGET_FOCUS |  |  |
722 | TARGET_SURFACE_ CROSSHAIR_HEIGHT |  |  |
499 | TARGET_SURFACE_DURATION |  |  |
497 | TARGET_SURFACE_HEIGHT |  |  |
501 | TARGET_SURFACE_HIACC |  |  |
490 | TARGET_SURFACE_ILLUM |  |  |
500 | TARGET_SURFACE_MODE |  |  |
498 | TARGET_SURFACE_RANGE |  |  |
511 | TARGET_SURFACE_TYPE |  |  |
496 | TARGET_SURFACE_WIDTH |  |  |
564 | TARGET_TYPE |  |  |
124 | TARGSLOT_I | Target slot vector i |  |
125 | TARGSLOT_J | Target slot vector j |  |
126 | TARGSLOT_K | Target slot vector k |  |
532 | TEMPP | Current Part temperature |  |
529 | TEMPX | Current X axis temperature |  |
530 | TEMPY | Current Y axis temperature |  |
531 | TEMPZ | Current Z axis temperature |  |
163 | TEXT_ANALSYIS | Use text analysis on dimension (Yes / No) |  |
761 | TEXTANAL_LABEL_DEV |  |  |
758 | TEXTANAL_LABEL_MEAS_I |  |  |
759 | TEXTANAL_LABEL_MEAS_J |  |  |
760 | TEXTANAL_LABEL_MEAS_K |  |  |
755 | TEXTANAL_LABEL_MEAS_X |  |  |
756 | TEXTANAL_LABEL_MEAS_Y |  |  |
757 | TEXTANAL_LABEL_MEAS_Z |  |  |
762 | TEXTANAL_LABEL_MINMAX |  |  |
566 | THEO_A |  |  |
609 | THEO_A2 | For CMT characteristic point 1 |  |
38 | THEO_ANGLE | Theoretical angle |  |
720 | THEO_AREA |  |  |
555 | THEO_DEPTH |  |  |
34 | THEO_DIAM | Theoretical diameter |  |
578 | THEO_EA |  |  |
579 | THEO_EH |  |  |
284 | THEO_END_ANG | Vision Circle Feature |  |
577 | THEO_ER |  |  |
13 | THEO_EX | Theoretical x - end point |  |
14 | THEO_EY | Theoretical y - end point |  |
15 | THEO_EZ | Theoretical z - end point |  |
551 | THEO_FLUSH |  |  |
553 | THEO_GAP |  |  |
567 | THEO_H |  |  |
610 | THEO_H2 | For CMT characteristic point 1 |  |
37 | THEO_HEIGHT | Theoretical height |  |
16 | THEO_I | Hit point theoretical i - vector | point number | Numeric value
17 | THEO_J | Hit point theoretical j - vector | point number | Numeric value
18 | THEO_K | Hit point theoretical k - vector | point number | Numeric value
36 | THEO_LENGTH | Theoretical length |  |
130 | THEO_MINOR_AXIS | Theoretical minor access |  |
718 | THEO_PERIMETER |  |  |
565 | THEO_R |  |  |
608 | THEO_R2 | For CMT characteristic point 1 |  |
575 | THEO_SA |  |  |
576 | THEO_SH |  |  |
574 | THEO_SR |  |  |
283 | THEO_START_ANG | Vision Circle Feature |  |
10 | THEO_SX | Theoretical x - start point |  |
11 | THEO_SY | Theoretical y - start point |  |
12 | THEO_SZ | Theoretical z - start point |  |
35 | THEO_WIDTH | Theoretical width |  |
7 | THEO_X | Hit point theoretical x - centroid | point number | X-Coordinate
393 | THEO_X2 | For CMT characteristic point 1 |  |
8 | THEO_Y | Hit point theoretical y - centroid | point number | Y-Coordinate
394 | THEO_Y2 | For CMT characteristic point 1 |  |
9 | THEO_Z | Hit point theoretical z - centroid | point number | Z-Coordinate
395 | THEO_Z2 | For CMT characteristic point 1 |  |
49 | THEOBF_TYPE | Use theoretical values for best fit algorithm (yes / no) |  |
41 | THICKNESS_TYPE | Theoretical or actual thickness | 0 | "THICKNESS_ NONE", "THEO_ THICKNESS", or "ACTL_ THICKNESS"
594 | THICKNESS_TYPE_EDGE | Theoretical or actual thickness |  |
67 | THINNING_TOL | Thinning tolerance for curves |  |
488 | THRESHOLD |  |  |
450 | TIME_ARG | For SPC |  |
401 | TIME_FILTER | For SPC: filtering based on time stamps |  |
229 | TIP_I | Tip shank vector i component |  |
230 | TIP_J | Tip shank vector j component |  |
231 | TIP_K | Tip shank vector k component |  |
418 | TITLE | For SPC |  |
349 | TOOL_DIAM | Tool diameter |  |
346 | TOOL_X | Tool x value |  |
347 | TOOL_Y | Tool y value |  |
348 | TOOL_Z | Tool z value |  |
169 | TP_MODIFIER | Dimension Position modifier |  |
726 | TP_MODIFIER2 | This is because TP_MODIFIER and TP_MODIFIER2 are used in two different groups in summary mode. |  |
400 | TRACE_FILTER | For SPC: filtering based on trace fields |  |
451 | TRACE_FILTER_ARG | For SPC |  |
257 | TRACE_NAME | Trace field name |  |
258 | TRACE_VALUE | Trace field value |  |
473 | TRACE_VALUE_LIMIT | Trace command character limit for the value field |  |
255 | TRANSFER_DIR | Transfer directory for statistics object |  |
212 | TRIGGER_FORCE | Trigger force for option probe object |  |
469 | TRIGGERPLANE |  |  |
463 | TRIGGERTOLERANCE |  |  |
464 | TRIGGERTOLVALUE |  |  |
131 | TWO_D_THREE_D_TYPE | 2d or 3d |  |

-S-

Number | Data Type Name | Data Type Description | Index | Value String
151 | SAVE_ALIGN_CAD_TO_PARTS | Save Align Save Type |  |
92 | SCAN_ACCELERATION | Scan acceleration |  |
265 | SCAN_AXISVEC_I | Axis vector i - for boundary conditions... |  |
266 | SCAN_AXISVEC_J | Axis vector j - for boundary conditions... |  |
267 | SCAN_AXISVEC_K | Axis vector k - for boundary conditions... |  |
432 | SCAN_BNDRY_TYPE |  |  |
274 | SCAN_CROSS_TOTAL | Number of crossings allowed in boundary condition |  |
259 | SCAN_CUTPLANEVEC_I | Cut plane vector i |  |
260 | SCAN_CUTPLANEVEC_J | Cut plane vector j |  |
261 | SCAN_CUTPLANEVEC_K | Cut plane vector k |  |
217 | SCAN_DENSITY | Scan density for option probe object |  |
276 | SCAN_EDGE_THICK | Edge thickness for edge scans |  |
268 | SCAN_ENDVEC_I | End touch vector i |  |
269 | SCAN_ENDVEC_J | End touch vector j |  |
270 | SCAN_ENDVEC_K | End touch vector k |  |
271 | SCAN_INITDIR_I | Unit direction vector i |  |
272 | SCAN_INITDIR_J | Unit direction vector j |  |
273 | SCAN_INITDIR_K | Unit direction vector k |  |
262 | SCAN_INITVEC_I | Initial touch vector i |  |
263 | SCAN_INITVEC_J | Initial touch vector j |  |
264 | SCAN_INITVEC_K | Initial touch vector k |  |
93 | SCAN_OFFSET_FORCE | Scan offset force |  |
358 | SCAN_TECHNIQUE | Scan technique |  |
275 | SCAN_TIME_INCR | Time increment for manual scans |  |
540 | SCREEN_CAPTURE_AUTO_TIME | Screen capture time (always or on error) |  |
536 | SCREEN_CAPTURE_AUTO_TYPE | Screen capture auto type (which gives more options that basic screen capture) |  |
503 | SCREEN_CAPTURE_QUALITY | Screen capture image color depth |  |
502 | SCREEN_CAPTURE_SCALE | Screen capture image size |  |
535 | SCREEN_CAPTURE_TYPE | Screen capture type (can now do Live Image View as well as CAD) |  |
57 | SEARCHMODE_TYPE | Box or circular search mode for hipoint feature |  |
764 | SECTION_INDEX |  |  |
225 | SENSOR_LIST | Sensor list for temp comp object |  |
193 | SERIAL_NUMBER | File header serial number |  |
494 | SHOW_COLUMN |  |  |
136 | SHOW_DETAILS | Display details for alignments and scans |  |
179 | SHOW_HEADINGS | Dimension format headings toggle |  |
135 | SHOW_IDS | Display id for alignments and loops |  |
414 | SHOW_MORE_SPC_CALCS | For SPC |  |
723 | SHOW_NOMS |  |  |
728 | SHOW_OPTIONS |  |  |
187 | SHOW_POINT_INFO | Point info / Show point info |  |
493 | SHOW_ROW |  |  |
402 | SHOW_SPC_CALCS | For SPC |  |
763 | SIMULT_EVAL |  |  |
235 | SINGLE_POINT | Point mode on dcc scan object |  |
145 | SKIP_NUM | Skip number of loop |  |
53 | SLOT_MIN_MAX_TYPE | Measure slot using 5 (NORM) or 6 (MINMAX) hits |  |
297 | SLOT_NUMBER | Sets the column slot number for a column load and unload |  |
563 | SLOT_TYPE |  |  |
109 | SLOTVEC_I | Slot vector i |  |
110 | SLOTVEC_J | Slot vector j |  |
111 | SLOTVEC_K | Slot vector k |  |
43 | SNAP_TYPE | Vector features / Surface features |  |
416 | SOLID | For SPC |  |
403 | SPEC_LIMITS | For SPC |  |
415 | SPEC_OFFSET | For SPC |  |
134 | SRC_EXPR | Source expression (assign, subroutine, call sub, basic script, flow control) |  |
181 | STANDARD_DEVIATION | Dimension format std dev toggle |  |
98 | START_ANG | Start angle | 0 | Radian value
466 | START_LABEL |  |  |
143 | START_NUM | Start number for loop |  |
254 | STAT_CALC_TYPE | Calc type on/off toggle for statistics object |  |
194 | STAT_COUNT | File header statistics count |  |
253 | STAT_NAME_TYPE | Variable name type for statistics object |  |
1 | STATIC_TOGGLE | Used for toggle fields that cannot contain expressions |  |
391 | STATS_DATASOURCE | Datasource for statistics object |  |
453 | STATS_DB_TYPE | For stats command database option |  |
248 | STATS_DIR | Stats directory for statistics object |  |
247 | STATS_TYPE | Stats type for statistics object |  |
405 | STDDEV | For spc |  |
195 | SUB_NAME | Subroutine name |  |
690 | SUMMARY_AXIS |  |  |
781 | SUMMARY_BONUS |  |  |
684 | SUMMARY_COLUMN_HDR |  |  |
640 | SUMMARY_DEV |  |  |
685 | SUMMARY_FEAT |  |  |
779 | SUMMARY_MAX |  |  |
692 | SUMMARY_MEAS |  |  |
780 | SUMMARY_MIN |  |  |
778 | SUMMARY_MINUSTOL |  |  |
691 | SUMMARY_NOMINAL |  |  |
776 | SUMMARY_OUTTOL |  |  |
777 | SUMMARY_PLUSTOL |  |  |
689 | SUMMARY_TBLHDR |  |  |
484 | SURFACE |  |  |
112 | SURFVEC_I | Surface vector i |  |
113 | SURFVEC_J | Surface vector j |  |
114 | SURFVEC_K | Surface vector k |  |
546 | SURFVEC_MEAS_I | Surface vector i meas |  |
547 | SURFVEC_MEAS_J | Surface vector j meas |  |
548 | SURFVEC_MEAS_K | Surface vector k meas |  |

-R-

Number | Data Type Name | Data Type Description | Index | Value String
171 | RADIUS_TYPE | Dimension 2D Distance radius type |  |
196 | READ_WRITE | Read / Write toggle |  |
46 | READPOS_TYPE | Read Position (yes / no) |  |
3 | REF_ID | ID of object being referred to |  |
222 | REF_TEMP | Reference temperature for temp comp object |  |
412 | REGR | For SPC |  |
142 | REPIERCE_CAD | Flag for iterative alignments |  |
383 | REPORT_SURFVEC_I | Extended sheet metal vector for DCC Edge |  |
384 | REPORT_SURFVEC_J | Extended sheet metal vector for DCC Edge |  |
385 | REPORT_SURFVEC_K | Extended sheet metal vector for DCC Edge |  |
121 | REPORTVEC_I | Report vector i |  |
122 | REPORTVEC_J | Report vector j |  |
123 | REPORTVEC_K | Report vector k |  |
188 | RET_ONLY_TYPE | Retrolinear only on / off toggle |  |
216 | RETURN_SPEED | Return speed for option probe object |  |
192 | REVISION_NUMBER | File header revision number |  |
48 | RMEAS_TYPE | Use relative measures (yes / no) |  |
69 | RMEASFEATID | Name of rmeas feature |  |
524 | RMEASFEATIDX | Referenced feature (X axis) | 0 | Feature lable
525 | RMEASFEATIDY | Referenced feature (Y axis) | 0 | Feature lable
526 | RMEASFEATIDZ | Referenced feature (Z axis) | 0 | Feature lable
5 | ROTATE_REF_ID | Ref id for a rotate feature of an iterative alignment |  |
158 | ROTATION_TYPE | Move rotary table type |  |
286 | ROW_ID |  |  |
639 | RPT_DIMENSION_TABLES |  |  |

-Q-

Number | Data Type Name | Data Type Description | Index | Value String
470 | QUERY_SHOW_GRAPHIC_SETTINGS |  |  |

-P-

Number | Data Type Name | Data Type Description | Index | Value String
374 | _PRINT_TO_FILE | Prepended with _ to avoid confusion with Edit window constants |  |
375 | _PRINT_TO_PRINTER | Prepended with _ to avoid confusion with Edit window constants |  |
191 | PART_NAME |  |  |
519 | PATTERN_TYPE | Auto plane pattern | 0 | "SQUARE" or "RADIAL"
487 | PERCENTAGE |  |  |
73 | PERM_HITS | Number of Perm (sample) hits | 0 | 0 or more
170 | PERP_PARALLEL_TYPE | Dimension perindicular parallel type |  |
115 | PINVEC_I | Pin vector i |  |
116 | PINVEC_J | Pin vector j |  |
117 | PINVEC_K | Pin vector k |  |
605 | PIXEL_TOGGLE |  |  |
186 | POINT_INFO_HEADING | Point info heading type |  |
380 | POINTINFO_FILTER_DEVIATION | Toggle field for deviation filter state of point info commands |  |
381 | POINTINFO_FILTER_ DEVIATION_NUMBER | Number field associated with deviation filter state of point info commands |  |
301 | POINTINFO_FILTER_INTERVAL | Toggle field for interval filter state of point info commands |  |
302 | POINTINFO_FILTER_ INTERVAL_NUMBER | Number field associated with interval filter state of point info commands |  |
382 | POINTINFO_FILTER_OUTTOL | Toggle field for outtol filter state of point info commands |  |
378 | POINTINFO_FILTER_WORST | Toggle field for worst filter state of point info commands |  |
379 | POINTINFO_FILTER_ WORST_NUMBER | Number field associated with worst filter state of point info commands |  |
218 | POLAR_VECTOR_COMPENSATION | Polar vector compensation object |  |
277 | POS_REPORT_AXIS_X | Positive reporting axis |  |
278 | POS_REPORT_AXIS_Y | Positive reporting axis |  |
279 | POS_REPORT_AXIS_Z | Positive reporting axis |  |
462 | POS_REPT_DISPLAY_OPTION |  |  |
214 | POSITIONAL_ACCURACY | Positional accuracy for option probe object |  |
786 | PPAP_INDEX |  |  |
399 | PPROG | Part program name (used in a database query) |  |
175 | PRECISION | Dimension display precision |  |
377 | PRINT_DELETE_RUNS |  |  |
376 | PRINT_DRAFTMODE |  |  |
213 | PROBE_ACCURACY | Probe accuracy for option probe object |  |
228 | PROBE_COMP | Probe comp (on/off) toggle |  |
299 | PROBING_MODE | Probing mode for option probe |  |
174 | PROFILE_FORM_TYPE | Dimension profile form type toggle |  |
550 | PROFILE_TYPE |  |  |
521 | PROGRAM_GAGE_FEAT_TYPE |  |  |
522 | PROGRAM_GAGE_TYPE |  |  |
118 | PUNCHVEC_I | Punch vector i |  |
119 | PUNCHVEC_J | Punch vector j |  |
120 | PUNCHVEC_K | Punch vector k |  |

-O-

Number | Data Type Name | Data Type Description | Index | Value String
61 | OFFSET_LINE_METHOD | method for offset lines |  |
238 | OFFSET_TOLERANCE | offset tolerance for perimeter scans |  |
156 | OLD_TIP | old tip in move ph9 offset |  |
285 | ONOFF_TYPE | Initially implemented for use with IGNOREROTAB but can be used with any ON OFF toggle field |  |
620 | OPERTYPE |  |  |
220 | ORIGIN | Origin data point for temp comp object |  |
6 | ORIGIN_REF_ID | Ref id for an origin feature of an iterative alignment |  |
449 | OUTPUT_DMIS_REPORT | DMO reporting |  |
448 | OUTPUT_FEAT_W_DIMENS | DMO reporting |  |
447 | OUTPUT_FEATURE_NOMS | DMO reporting |  |
165 | OUTPUT_TYPE | Mode of output for dimensions |  |
558 | OVERLAP |  |  |
559 | OVERSCAN |  |  |
446 | OVERWRITE | DMO reporting |  |

-N-

Number | Data Type Name | Data Type Description | Index | Value String
429 | N_CONTROLPOINTS | Number of control points in a scan |  |
70 | N_HITS | Number of hits per row | 0 | 1 or more
55 | N_INIT_HITS_TYPE | Toggle field for fixed number of init hits |  |
56 | N_PERM_HITS_TYPE | Toggle field for fixed number of perm hits |  |
71 | N_ROWS | Number of rows | 0 | 1 or more
489 | N_SIDES | Number of polygon sides |  |
249 | NEW_STATS_DIR | Empty stats dir field in editor for statistics object |  |
157 | NEW_TIP | New tip in move ph9 offset |  |
0 | NINGUNO_TIPO | No type, default value, used with constants |  |
826 | NO_APPROACH_VECTOR_FLIP | Allow the feature vector to be flipped during optimzation | 0 | "YES" or "NO"
482 | NOFLIPFLIP_CONFIG |  |  |
166 | NOMINAL | Dimension nominal value |  |
321 | NOMINAL_COLOR | Vision Nominal Color |  |
232 | NORM_RELEARN | Normal scan mode or re-learn nominals mode |  |
317 | NUM_CONTROL_POINTS | Number of control points |  |
320 | NUM_FIT_POINTS | Number of points used for fitting surface |  |
356 | NUM_ITERATIONS | Number of iterations |  |
215 | NUM_RETURN_DATA | Return data for option probe object |  |

-M-

Number | Data Type Name | Data Type Description | Index | Value String
227 | MACHINE_TYPE | Machine type for load machine object |  |
485 | MAGNIFICATION |  |  |
176 | MAN_RETRACT |  |  |
94 | MANUAL_FINE_PROBING | Manual fine probing |  |
534 | MANUAL_PREPOSITION | Whether manual pre-position needed on vision target |  |
221 | MATERIAL_COEFFICIENT | Material coefficient for temp comp object |  |
242 | MAX_ANGLE | Setting for variable technique on scans |  |
209 | MAX_FORCE | Max force for option probe object |  |
240 | MAX_INCREMENT | Setting for variable technique on scans |  |
491 | MEAN |  |  |
569 | MEAS_A |  |  |
612 | MEAS_A2 | For CMT characteristic point 1 |  |
30 | MEAS_ANGLE | Measured angle |  |
721 | MEAS_AREA |  |  |
556 | MEAS_DEPTH |  |  |
29 | MEAS_DIAM | Measured diameter |  |
584 | MEAS_EA |  |  |
585 | MEAS_EH |  |  |
624 | MEAS_END_ANG |  |  |
583 | MEAS_ER |  |  |
313 | MEAS_EX | Measured endpoint x component |  |
314 | MEAS_EY | Measured endpoint y component |  |
315 | MEAS_EZ | Measured endpoint z component |  |
552 | MEAS_FLUSH |  |  |
554 | MEAS_GAP |  |  |
570 | MEAS_H |  |  |
613 | MEAS_H2 | For CMT characteristic point 1 |  |
306 | MEAS_HEIGHT | Measured height |  |
25 | MEAS_I | Measured i |  |
26 | MEAS_J | Measured j |  |
27 | MEAS_K | Measured k |  |
28 | MEAS_LENGTH | Measured length |  |
305 | MEAS_MINOR_AXIS | Measured minor axis (ellipse) |  |
719 | MEAS_PERIMETER |  |  |
568 | MEAS_R |  |  |
611 | MEAS_R2 | For cmt characteristic point 1 |  |
581 | MEAS_SA |  |  |
582 | MEAS_SH |  |  |
307 | MEAS_SLOTVEC_I | Measured slot vector i |  |
308 | MEAS_SLOTVEC_J | Measured slot vector j |  |
309 | MEAS_SLOTVEC_K | Measured slot vector k |  |
580 | MEAS_SR |  |  |
623 | MEAS_START_ANG |  |  |
310 | MEAS_SX | Measured startpoint x component |  |
311 | MEAS_SY | Measured startpoint y component |  |
312 | MEAS_SZ | Measured startpoint z component |  |
316 | MEAS_WIDTH | Measured width |  |
22 | MEAS_X | Hit point measured x | point number | X-Coordinate
396 | MEAS_X2 | For CMT characteristic point 1 |  |
23 | MEAS_Y | Hit point measured y | point number | Y-Coordinate
397 | MEAS_Y2 | For CMT characteristic point 1 |  |
24 | MEAS_Z | Hit point measured z | point number | Z-Coordinate
398 | MEAS_Z2 | For CMT characteristic point 1 |  |
141 | MEASURE_ALL_FEATURES | Flag for iterative alignments |  |
59 | MEASURE_ORDER_TYPE | Measure order for edge feature SURFACE/ EDGE/ BOTH |  |
66 | MEASURED_2D3D_TYPE | Determines plane in which solution will lie or 3D solution |  |
106 | MEASVEC_I | Measure vector i |  |
107 | MEASVEC_J | Measure vector j |  |
108 | MEASVEC_K | Measure vector k |  |
357 | METHOD_TYPE | Scan method type |  |
100 | MIDPOINT_X | Midpoint x |  |
101 | MIDPOINT_Y | Midpoint y |  |
102 | MIDPOINT_Z | Midpoint z |  |
241 | MIN_ANGLE | Setting for variable technique on scans |  |
239 | MIN_INCREMENT | Setting for variable technique on scans |  |
486 | MINOR_WORD_TOGGLE |  |  |
58 | MODE_TYPE | MANUAL or DCC |  |
45 | MOVE_TYPE | Use auto move (yes / no) |  |

-L-

Number | Data Type Name | Data Type Description | Index | Value String
200 | LABEL_ID | Label field for flow control objects that reference labels |  |
729 | LEADER_LINE_ID |  |  |
480 | LEFTYRIGHTY_CONFIG |  |  |
4 | LEVEL_REF_ID | Ref id for a level feature of an iterative alignment |  |
62 | LIN_POL_FILT_TYPE | Filter object - linear or polar filter |  |
782 | LINE1_BONUS |  |  |
643 | LINE1_CALLOUT |  |  |
644 | LINE1_COLUMN_HDR |  |  |
650 | LINE1_DEV |  |  |
651 | LINE1_DEVPERCENT |  |  |
750 | LINE1_DEVPERCENT_NOM |  |  |
752 | LINE1_DEVPERCENT2 |  |  |
645 | LINE1_FEATNAME |  |  |
652 | LINE1_ISBILATERAL |  |  |
768 | LINE1_MAX |  |  |
647 | LINE1_MEAS |  |  |
769 | LINE1_MIN |  |  |
649 | LINE1_MINUSTOL |  |  |
646 | LINE1_NOMINAL |  |  |
653 | LINE1_NUMZONES |  |  |
765 | LINE1_OUTTOL |  |  |
648 | LINE1_PLUSTOL |  |  |
642 | LINE1_TBLHDR |  |  |
751 | LINE1_USE2DEVIATIONS |  |  |
686 | LINE2_AXIS |  |  |
658 | LINE2_BONUS |  |  |
655 | LINE2_CALLOUT |  |  |
656 | LINE2_COLUMN_HDR |  |  |
660 | LINE2_DATUMSHFT |  |  |
662 | LINE2_DEV |  |  |
663 | LINE2_DEVANG |  |  |
664 | LINE2_DEVPERCENT |  |  |
740 | LINE2_DEVPERCENT_NOM |  |  |
742 | LINE2_DEVPERCENT2 |  |  |
657 | LINE2_FEATNAME |  |  |
697 | LINE2_ISBILATERAL |  |  |
695 | LINE2_MAX |  |  |
688 | LINE2_MEAS |  |  |
696 | LINE2_MIN |  |  |
694 | LINE2_MINUSTOL |  |  |
687 | LINE2_NOMINAL |  |  |
698 | LINE2_NUMZONES |  |  |
766 | LINE2_OUTTOL |  |  |
693 | LINE2_PLUSTOL |  |  |
654 | LINE2_TBLHDR |  |  |
659 | LINE2_TOL |  |  |
661 | LINE2_UNUSEDZONE |  |  |
741 | LINE2_USE2DEVIATIONS |  |  |
669 | LINE3_BONUS |  |  |
666 | LINE3_CALLOUT |  |  |
667 | LINE3_COLUMN_HDR |  |  |
671 | LINE3_DATUMSHFT |  |  |
673 | LINE3_DEV |  |  |
674 | LINE3_DEVANG |  |  |
675 | LINE3_DEVPERCENT |  |  |
743 | LINE3_DEVPERCENT_NOM |  |  |
745 | LINE3_DEVPERCENT2 |  |  |
668 | LINE3_FEATNAME |  |  |
699 | LINE3_ISBILATERAL |  |  |
774 | LINE3_MAX |  |  |
771 | LINE3_MEAS |  |  |
775 | LINE3_MIN |  |  |
773 | LINE3_MINUSTOL |  |  |
770 | LINE3_NOMINAL |  |  |
700 | LINE3_NUMZONES |  |  |
767 | LINE3_OUTTOL |  |  |
772 | LINE3_PLUSTOL |  |  |
665 | LINE3_TBLHDR |  |  |
670 | LINE3_TOL |  |  |
672 | LINE3_UNUSEDZONE |  |  |
744 | LINE3_USE2DEVIATIONS |  |  |
355 | LOAD_TYPE | Load setting |  |
287 | LOCATOR_BMP | Feature Locator BMP On/Off |  |
288 | LOCATOR_WAV | Feature Locator WAV On/Off |  |
210 | LOW_FORCE | Low force for option probe object |  |
224 | LOW_THRESHOLD | Low threshold for temp comp object |  |

-K-

No Entries Available

-J-

No Entries Available

-I-

Number | Data Type Name | Data Type Description | Index | Value String
2 | ID | Object id |  |
392 | IGNOREMOTIONERRORS_TYPE | For ignore motion errors command |  |
205 | INDEX_END | Array index end number |  |
204 | INDEX_START | Array index start number |  |
72 | INIT_HITS | Initial hits |  |
40 | INOUT_TYPE | Inside / Outside |  |
596 | INTENSITY |  |  |
150 | INTERNAL_EXTERNAL | Recall Alignment |  |
454 | IOCHANNEL_NUMBER | For IO channel management commands |  |
457 | IOCHANNEL_PULSE_DURATION | No longer used, probably should be removed |  |
456 | IOCHANNEL_PULSE_INTERVAL | No longer used, probably should be removed |  |
455 | IOCHANNEL_PULSE_WIDTH | No longer used, probably should be removed |  |
634 | ISLAND_AI |  |  |
635 | ISLAND_AJ |  |  |
636 | ISLAND_AK |  |  |
638 | ISLAND_CLEARANCEDIST |  |  |
625 | ISLAND_DIAM |  |  |
631 | ISLAND_I |  |  |
632 | ISLAND_J |  |  |
633 | ISLAND_K |  |  |
626 | ISLAND_LENGTH |  |  |
637 | ISLAND_TYPE |  |  |
627 | ISLAND_WIDTH |  |  |
628 | ISLAND_X |  |  |
629 | ISLAND_Y |  |  |
630 | ISLAND_Z |  |  |
138 | ITEM_USED | Best fit item used in calculation of alignment |  |
354 | ITERATE_COLUMNS | Iterate columns setting |  |

-H-

Number | Data Type Name | Data Type Description | Index | Value String
483 | HIGH_ACCURACY |  |  |
223 | HIGH_THRESHOLD | High threshold for temp comp object |  |
407 | HISTOGRAM | For SPC |  |
359 | HIT_TYPE | Hit type |  |
68 | HITINT_TYPE | Interior/Exterior measurement flag |  |

-G-

Number | Data Type Name | Data Type Description | Index | Value String
183 | GAP_ONLY_TYPE | ON / OFF toggle |  |
708 | GDT_SYMBOL |  |  |
730 | GDT_SYMBOL2 |  |  |
64 | GEN_ALIGN_TYPE | Generic feature alignment type (independent / dependent) |  |
63 | GEN_FEAT_TYPE | Generic feature type |  |
162 | GRAPH_ANALYSIS | Use graphical analysis on dimension (yes / no) |  |
785 | GRAPH_ANALYSIS_MINUS_TOL | Auto Feature cad point minus tolerance |  |
784 | GRAPH_ANALYSIS_PLUS_TOL | Auto Feature cad point plus tolerance |  |
783 | GRAPH_ANALYSIS_POINT_SIZE | Auto Feature cad point size |  |
458 | GRAPH_OPTION | Dimension info and point info commands |  |
408 | GRID | For SPC |  |

-F-

Number | Data Type Name | Data Type Description | Index | Value String
79 | F_AUTOMOVE | Automove distance |  |
85 | F_BOXLENGTH |  |  |
84 | F_BOXWIDTH |  |  |
88 | F_CHECK | The only numeric associated with the CPCDcheck feature |  |
87 | F_CIRCRADIN |  |  |
86 | F_CIRCRADOUT |  |  |
81 | F_CORNER_RADIUS |  |  |
78 | F_DEPTH | Depth of measurements | 0 | Depth value
82 | F_INCREMENT |  |  |
80 | F_INDENT | Measurement offsets for various features | 1 | Offset value
243 | F_LOCATION | Location value for section scans |  |
89 | F_MAXACCELX | Maximum X acceleration |  |
90 | F_MAXACCELY | Maximum Y acceleration |  |
91 | F_MAXACCELZ | Maximum Z acceleration |  |
168 | F_MINUS_TOL | Dimension minus tol value |  |
95 | F_MOVESPEED | Move speed |  |
74 | F_OFFSET | Offset value |  |
76 | F_PITCH | Auto feature pitch |  |
167 | F_PLUS_TOL | Dimension plus tol value |  |
97 | F_SCANSPEED | Scan speed |  |
434 | F_SIZE | for SPC |  |
75 | F_SPACER | Auto feature spacer | 0 | Max distance value
77 | F_THICKNESS | Sheet metal thickness | 0 | Thickness value
593 | F_THICKNESS_EDGE |  |  |
83 | F_TOLERANCE |  |  |
96 | F_TOUCHSPEED | Touch speed |  |
208 | FAIL_ON_EXIST | File i/o fail on exist mode |  |
303 | FEAT_TYPE | Feature Type |  |
198 | FIELD_WIDTH | Field width for dmis file read/write command |  |
206 | FILE_COMMAND_TYPE | File i/o command type |  |
152 | FILE_NAME | File name |  |
197 | FILE_POINTER | File pointer name for file i/o commands |  |
598 | FILTER_NEIGHBOR_NUM |  |  |
606 | FILTER_TOGGLE |  |  |
600 | FILTER_TOL_ABOVE |  |  |
601 | FILTER_TOL_BELOW |  |  |
602 | FILTER_TOL_RIGHT |  |  |
472 | FILTER_TYPE | Basic scan filter type |  |
460 | FIND_HOLE_PERCENT | For the check command and find hole check distance |  |
54 | FIND_NOM_AXIS_TYPE | Selects between X, Y, Z, or user defined nominal axis |  |
233 | FIND_NOMS_TYPE | Type for find noms mode |  |
47 | FINDHOLE_TYPE | Use find hole algorithm (Yes / No) |  |
527 | FINDNOMS_BESTFIT |  |  |
528 | FINDNOMS_ONLYSELECTED |  |  |
452 | FIT |  |  |
465 | FIXTURE_TOL |  |  |
226 | FIXTURE_TYPE | Type for load fixture object |  |
246 | FLY_MODE_TYPE | Fly mode Off/On toggle |  |
560 | FREQUENCY |  |  |

-E-

Number | Data Type Name | Data Type Description | Index | Value String
99 | END_ANG | End angle | 0 | Radian value
144 | END_NUM | End number of loop |  |
787 | END_OFFSET | Ending depth | 0 | Ending depth value
467 | ERROR_LABEL |  |  |
202 | ERROR_MODE | Error mode for on error flow control command |  |
201 | ERROR_TYPE | Error type for on error flow control command |  |
292 | EXCLUSION_ZONE | Exclusion zone command is on or off |  |
293 | EXECUTE | Is the attached program executed (Yes / No) |  |
595 | EXPOSURE |  |  |

-D-

Number | Data Type Name | Data Type Description | Index | Value String
252 | DATA_MEM_PAGES | Database memory pages for statistics object |  |
250 | DATA_READ_LOCK | Database read lock for statistics object |  |
251 | DATA_WRITE_LOCK | Database write lock for statistics object |  |
731 | DATUM1_MODIFIER |  |  |
734 | DATUM1_MODIFIER2 |  |  |
725 | DATUM2 | This is because DATUM and DATUM2 are used in two different groups in summary mode. |  |
732 | DATUM2_MODIFIER |  |  |
735 | DATUM2_MODIFIER2 |  |  |
733 | DATUM3_MODIFIER |  |  |
736 | DATUM3_MODIFIER2 |  |  |
389 | DB_CHART_NAME | For SPC: chart name |  |
386 | DB_QUERY_OP | For SPC |  |
387 | DB_SOURCE_NAME | For SPC |  |
459 | DB_SOURCE_TYPE | For SPC |  |
539 | DELETE_TYPE | FILE/CLOSE, fptr, KEEP | DELETE |  |
203 | DESCRIPTION | Subroutine parameter description |  |
727 | DESCRIPTION2 | This is because DESCRIPTION and DESCRIPTION2 are used in two different groups in summary mode. |  |
133 | DEST_EXPR | Destination expressions (assign, subroutine, hyper report) |  |
353 | DEV_DIAM | Dev diam value |  |
280 | DEV_PERPEN_CENTERLINE |  |  |
350 | DEV_X | Dev x value |  |
351 | DEV_Y | Dev y value |  |
352 | DEV_Z | Dev z value |  |
390 | DEVIATION_ANGLE | Deviation angle |  |
180 | DEVIATION_SYMBOLS | Dimension format dev symbols toggle |  |
737 | DEVPERCENT_NOM |  |  |
739 | DEVPERCENT2 |  |  |
199 | DIGIT_COUNT | Digit count for dmis file read/write command |  |
324 | DIM_BONUS | Dimension bonus |  |
340 | DIM_DEVIATION | Dimension deviation |  |
182 | DIM_HEADING | Dimension format heading item |  |
304 | DIM_ID | For Best Fit 2d Alignments |  |
160 | DIM_INFO_LOC | Dimension info object location axis toggle |  |
159 | DIM_INFO_ORDER | Dimension info order toggle |  |
161 | DIM_INFO_TP_LOC | Dimension info object tp location axis toggle |  |
173 | DIM_LENGTH | Dimension length |  |
754 | DIM_LENGTH2 |  |  |
332 | DIM_MAX | Dimension max value |  |
328 | DIM_MEASURED | Measured dimension value |  |
336 | DIM_MIN | Dimension min value |  |
344 | DIM_OUTTOL | Dimension outtol |  |
703 | DIM_RPT_DATUM |  |  |
705 | DIM_RPT_DEVPERCENT |  |  |
704 | DIM_RPT_GRAPHIC |  |  |
706 | DIM_RPT_ISBILATERAL |  |  |
702 | DIM_RPT_ISDATUM |  |  |
707 | DIM_RPT_NUMZONES |  |  |
177 | DIM_TEXT | Dimension format dim text toggle |  |
178 | DIM_TEXT_OPTIONS | Dimension format dim text options toggle |  |
510 | DISPLAY_ADVANCED_PARAMETERS |  |  |
236 | DISPLAY_HITS | Scan flag (yes / no) for display of scan hits |  |
184 | DISPLAY_ID | Point info show id toggle |  |
607 | DISPLAY_PROBE_PARAMETERS |  |  |
256 | DISPLAY_TRACE | Trace field object yes/no toggle for dialog display |  |
185 | DISPLAY_TYPE | Point info show type toggle |  |
155 | DISTANCE | Distance |  |
676 | DRF_COLUMN_HDR |  |  |
681 | DRF_ROTATIONX |  |  |
682 | DRF_ROTATIONY |  |  |
683 | DRF_ROTATIONZ |  |  |
677 | DRF_SEGNAME |  |  |
678 | DRF_SHIFTX |  |  |
679 | DRF_SHIFTY |  |  |
680 | DRF_SHIFTZ |  |  |
641 | DRF_TBLHDR |  |  |
291 | DTYPE_LEAPFROGFULLPARTIAL | Leapfrog type: Full leapfrog or partial leapfrog |  |
290 | DTYPE_LEAPFROGNUMHITS | Number of hits to be taken during leapfrog procedure |  |
289 | DTYPE_LEAPFROGTYPE | Type of leapfrog being performed |  |

-C-

Number | Data Type Name | Data Type Description | Index | Value String
492 | CAD_COMP |  |  |
237 | CAD_TOLERANCE | CAD tolerance for perimeter scans |  |
471 | CALC_STYLE_FILE |  |  |
413 | CENTER_POINT | For SPC |  |
478 | CENTER_ROTATION_MEAS | Best fit alignments |  |
477 | CENTER_ROTATION_THEO | Best fit alignments |  |
445 | CHART_SUB_TYPE | For SPC |  |
388 | CHART_TYPE | For SPC: charts |  |
42 | CIRC_TYPE | Circular or straight probe motion (circles and cylinders) |  |
614 | CLIP_LEFT_DIST |  |  |
604 | CLIP_LOW_DIST |  |  |
615 | CLIP_RIGHT_DIST |  |  |
603 | CLIP_UP_DIST |  |  |
244 | COL132_TYPE | On / Off setting for column 132 object |  |
701 | COLUMN_HDR |  |  |
296 | COLUMN_ID | Sets the column id for a load or unload column command |  |
245 | COMMAND_STRING | For external command object |  |
189 | COMMENT | Comment text |  |
709 | COMMENT_INPUT | Add new type for comment input value |  |
190 | COMMENT_TYPE | Comment type |  |
724 | COMPOSITE |  |  |
468 | CONE_CONVEX_TYPE |  |  |
60 | CONE_LENGTH_ANGLE_TYPE | For cones: show length or angle |  |
39 | COORD_TYPE | Coordinate System |  |
621 | COP_BOOLEANTYPE |  |  |
618 | COP_COLORMAP |  |  |
619 | COP_COPLEMENT |  |  |
616 | COP_EXPORTFILETYPE |  |  |
543 | COP_FILTER |  |  |
622 | COP_IMPORTFILETYPE |  |  |
617 | COP_SELECTIONTYPE |  |  |
544 | COP_SIZE |  |  |
545 | COP_TYPE |  |  |
425 | CPOINT_DIAM |  |  |
428 | CPOINT_F_SCANSPEED |  |  |
422 | CPOINT_I |  |  |
423 | CPOINT_J |  |  |
424 | CPOINT_K |  |  |
426 | CPOINT_SCAN_CROSS_TOTAL |  |  |
427 | CPOINT_SCAN_DENSITY |  |  |
430 | CPOINT_TYPE |  |  |
419 | CPOINT_X |  |  |
420 | CPOINT_Y |  |  |
421 | CPOINT_Z |  |  |
433 | CREATE_WEIGHTS | For best fit 2D/3D alignments |  |
65 | CURVE_TYPE | For curves - type of curve |  |

-B-

Number | Data Type Name | Data Type Description | Index | Value String
51 | BF_MATH_TYPE | Math type used to calculate best fit |  |
50 | BOUND_TYPE | Bound / Unbound |  |
360 | BOUNDARY_POINT_X | Boundary Point x |  |
361 | BOUNDARY_POINT_Y | Boundary point y |  |
362 | BOUNDARY_POINT_Z | Boundary point z |  |
476 | BSMETHOD_TYPE |  |  |
207 | BUFFER_SIZE_TYPE | File i/o buffer size |  |

-A-

Number | Data Type Name | Data Type Description | Index | Value String
481 | ABOVEBELOW_CONFIG |  |  |
409 | ADDITIONAL_CHART | For SPC |  |
153 | ALIGN_LIST | Show alignment in alignment list (Yes / No) |  |
300 | ANGLE_COMP_TOGGLE | Toggle field for complement state of angle dimensions |  |
149 | ANGLE_OFFSET | Angle Offset for loops and rotary tables |  |
373 | ANGULARITY_NOM_ANGLE | The reference angle used, not the dimension's nominal |  |
103 | ANGVEC_I | Angle vector i | 0 | Numeric value
104 | ANGVEC_J | Angle vector j | 0 | Numeric value
105 | ANGVEC_K | Angle vector k | 0 | Numeric value
164 | ARROW_MULTIPLIER | Dimension arrow multiplier value |  |
479 | ARTICULATEDARM_TYPE |  |  |
234 | AUTO_CLEAR_PLANE | Auto clear plane flag |  |
461 | AUTO_ONERROR_TYPE |  |  |
533 | AUTO_PH9 |  |  |
219 | AUTO_PRINT | Auto print flag for hyper report object |  |
295 | AUTOBEEPING | Turn autotrigger beeping on/off |  |
52 | AUTOFIT_CONSTRAINT | Toggle for type of constraint on best fit alignment |  |
298 | AUTOTOLZONE | Tolerance zone for autotrigger |  |
294 | AUTOTRIGGERONOFF | Turn autotrigger on or off. |  |
140 | AVERAGE_ERROR | Flag for iterative alignments |  |
749 | AXIS_DESCRIPTION |  |  |
747 | AXIS_MINUS_TOL |  |  |
132 | AXIS_NOMINAL | Axis |  |
748 | AXIS_NOMINAL |  |  |
746 | AXIS_PLUS_TOL |  |  |