## Dimensioning through Keyboard Input

Looking for XactMeasure GD&T dimensions? If so, see:

- Using Feature Control Frames
- GD&T Dialog Box

Dimensional Keyin dialog box

The Insert | Dimension | Keyin menu option allows you to capture and "key in" through the keyboard data not measured with the CMM (for instance, adding a dimension that is measured with calipers). This option allows you to print out all inspection results on the inspection report (not just features measured with the CMM). It is also useful when collecting data for statistical analysis.

More:

To Add Dimensions Using the KEY IN Option:

Nominal

Actual

Tolerances for Keyboard Created Dimensions