#### Setting Boundary Points Using the Measured Point Method

To set the boundary of the scan using measured points, touch the probe on the part. This will automatically update the value of the Boundary point that is currently selected in the Boundary list. The focus will then move to the next boundary point (if there are any in the list). In the case of a PATCH scan, an extra boundary point will be added automatically if the current point is the last point in the list. The PATCH scan will display the last point (this is the same as the previous point). PC-DMIS will delete this last point when the OK button is selected in the dialog box.